{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["信息公开"],"not_rendered":{"images":4},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"信息公开","index":0,"n_rows":663,"n_cols":16,"rows_kept":663,"merged":[[1,0,1,3],[2,0,2,3],[3,0,3,3],[4,0,4,2],[4,3,4,7],[5,0,5,2],[5,3,5,7],[6,0,6,2],[6,3,6,7],[7,0,7,2],[7,3,7,7],[8,0,8,2],[8,3,8,7],[9,0,9,2],[9,3,9,7],[10,0,10,2],[10,3,10,7],[11,0,11,2],[11,3,11,7],[12,0,12,2],[12,3,12,7],[13,0,13,2],[13,3,13,7],[14,0,14,2],[14,3,14,7],[15,0,15,2],[15,3,15,7],[16,0,16,2],[16,3,16,7],[17,0,17,2],[17,3,17,7],[18,0,18,2],[18,3,18,7],[19,0,19,2],[19,3,19,7],[20,0,20,2],[20,3,20,7],[21,0,21,2],[22,0,23,0],[22,1,23,1],[22,2,23,2],[22,3,23,3],[22,4,23,4],[22,5,22,8],[22,9,23,9],[22,10,23,10],[22,11,23,11],[22,12,23,12],[22,13,23,13],[22,14,23,14],[22,15,23,15],[24,0,88,0],[24,1,32,1],[24,2,32,2],[24,9,32,9],[24,10,32,10],[24,11,32,11],[24,12,32,12],[24,13,32,13],[24,14,32,14],[24,15,32,15],[33,1,34,1],[33,2,34,2],[33,9,34,9],[33,10,34,10],[33,11,34,11],[33,12,88,12],[33,13,34,13],[33,14,34,14],[33,15,34,15],[35,1,37,1],[35,2,37,2],[35,9,37,9],[35,10,37,10],[35,11,37,11],[35,13,37,13],[35,14,37,14],[35,15,37,15],[38,1,64,1],[38,2,64,2],[38,9,64,9],[38,10,64,10],[38,11,64,11],[38,13,64,13],[38,14,64,14],[38,15,64,15],[65,1,82,1],[65,2,82,2],[65,9,82,9],[65,10,82,10],[65,11,82,11],[65,13,82,13],[65,14,82,14],[65,15,82,15],[83,1,85,1],[83,2,85,2],[83,9,85,9],[83,10,85,10],[83,11,85,11],[83,13,85,13],[83,14,85,14],[83,15,85,15],[86,1,88,1],[86,2,88,2],[86,9,88,9],[86,10,88,10],[86,11,88,11],[86,13,88,13],[86,14,88,14],[86,15,88,15],[89,0,117,0],[89,1,96,1],[89,2,96,2],[89,9,96,9],[89,10,96,10],[89,11,96,11],[89,12,96,12],[89,13,96,13],[89,14,96,14],[89,15,96,15],[97,1,102,1],[97,2,102,2],[97,9,102,9],[97,10,102,10],[97,11,102,11],[97,12,161,12],[97,13,102,13],[97,14,102,14],[97,15,102,15],[103,1,106,1],[103,2,106,2],[103,9,106,9],[103,10,106,10],[103,11,106,11],[103,13,106,13],[103,14,106,14],[103,15,106,15],[107,1,108,1],[107,2,108,2],[107,9,108,9],[107,10,108,10],[107,11,108,11],[107,13,108,13],[107,14,108,14],[107,15,108,15],[109,1,111,1],[109,2,111,2],[109,9,111,9],[109,10,111,10],[109,11,111,11],[109,13,111,13],[109,14,111,14],[109,15,111,15],[112,1,114,1],[112,2,114,2],[112,9,114,9],[112,10,114,10],[112,11,114,11],[112,13,114,13],[112,14,114,14],[112,15,114,15],[115,1,117,1],[115,2,117,2],[115,9,117,9],[115,10,117,10],[115,11,117,11],[115,13,117,13],[115,14,117,14],[115,15,117,15],[118,0,161,0],[118,1,122,1],[118,2,122,2],[118,9,122,9],[118,10,122,10],[118,11,122,11],[118,13,122,13],[118,14,122,14],[118,15,122,15],[124,1,148,1],[124,2,148,2],[124,9,148,9],[124,10,148,10],[124,11,148,11],[124,13,148,13],[124,14,148,14],[124,15,148,15],[149,1,152,1],[149,2,152,2],[149,9,152,9],[149,10,152,10],[149,11,152,11],[149,13,152,13],[149,14,152,14],[149,15,152,15],[153,1,157,1],[153,2,157,2],[153,9,157,9],[153,10,157,10],[153,11,157,11],[153,13,157,13],[153,14,157,14],[153,15,157,15],[158,1,159,1],[158,2,159,2],[158,9,159,9],[158,10,159,10],[158,11,159,11],[158,13,159,13],[158,14,159,14],[158,15,159,15],[163,0,164,0],[163,1,164,1],[163,2,164,2],[163,3,164,3],[163,4,164,4],[163,5,163,6],[163,7,163,8],[163,9,164,9],[163,10,164,10],[163,11,164,12],[165,11,165,12],[166,0,167,0],[166,1,167,1],[166,2,167,2],[166,11,166,12],[167,11,167,12],[168,11,168,12],[170,0,171,0],[170,1,171,1],[170,2,171,2],[170,3,171,3],[170,4,171,4],[170,5,171,5],[170,6,171,6],[170,7,170,10],[170,11,171,11],[170,12,171,12],[172,0,178,0],[172,1,178,1],[172,2,178,2],[172,3,173,3],[172,4,173,4],[172,12,173,12],[174,3,175,3],[174,4,175,4],[174,12,175,12],[177,3,178,3],[177,4,178,4],[177,12,178,12],[179,0,228,0],[179,1,228,1],[179,2,228,2],[179,3,190,3],[179,4,190,4],[179,12,190,12],[193,3,194,3],[193,4,194,4],[193,12,194,12],[195,3,206,3],[195,4,206,4],[195,12,206,12],[208,3,211,3],[208,4,211,4],[208,12,211,12],[212,3,215,3],[212,4,215,4],[212,12,215,12],[216,3,219,3],[216,4,219,4],[216,12,219,12],[220,3,224,3],[220,4,224,4],[220,12,224,12],[225,3,228,3],[225,4,228,4],[225,12,228,12],[229,0,234,0],[229,1,234,1],[229,2,234,2],[229,3,230,3],[229,4,230,4],[229,12,230,12],[235,0,235,2],[236,0,236,2],[237,0,237,3],[238,0,239,0],[238,1,239,1],[238,2,239,4],[238,5,238,6],[238,7,239,7],[238,9,239,9],[238,10,239,10],[240,2,240,4],[241,2,241,4],[242,0,242,3],[243,0,244,0],[243,1,244,1],[243,2,244,2],[243,3,243,8],[243,9,244,9],[243,10,244,11],[243,12,244,13],[244,3,244,6],[245,3,245,6],[245,10,245,11],[245,12,245,13],[246,3,246,6],[246,10,246,11],[246,12,246,13],[247,3,247,6],[247,10,247,11],[247,12,247,13],[248,3,248,6],[248,10,248,11],[248,12,248,13],[249,3,249,6],[249,10,249,11],[249,12,249,13],[250,3,250,6],[250,10,250,11],[250,12,250,13],[251,3,251,6],[251,10,251,11],[251,12,251,13],[252,3,252,6],[252,10,252,11],[252,12,252,13],[253,3,253,6],[253,10,253,11],[253,12,253,13],[254,3,254,6],[254,10,254,11],[254,12,254,13],[255,3,255,6],[255,10,255,11],[255,12,255,13],[256,3,256,6],[256,10,256,11],[256,12,256,13],[257,3,257,6],[257,10,257,11],[257,12,257,13],[258,3,258,6],[258,10,258,11],[258,12,258,13],[259,3,259,6],[259,10,259,11],[259,12,259,13],[260,3,260,6],[260,10,260,11],[260,12,260,13],[261,3,261,6],[261,10,261,11],[261,12,261,13],[262,3,262,6],[262,10,262,11],[262,12,262,13],[263,3,263,6],[263,10,263,11],[263,12,263,13],[264,3,264,6],[264,10,264,11],[264,12,264,13],[265,0,265,3],[266,0,266,3],[267,0,268,0],[267,1,268,1],[267,2,268,2],[267,3,268,3],[267,4,268,4],[267,5,267,9],[267,10,268,11],[267,12,268,13],[269,10,269,11],[269,12,269,13],[270,10,270,11],[270,12,270,13],[271,10,271,11],[271,12,271,13],[272,10,272,11],[272,12,272,13],[273,10,273,11],[273,12,273,13],[274,10,274,11],[274,12,274,13],[275,10,275,11],[275,12,275,13],[276,10,276,11],[276,12,276,13],[277,10,277,11],[277,12,277,13],[278,10,278,11],[278,12,278,13],[279,10,279,11],[279,12,279,13],[280,10,280,11],[280,12,280,13],[281,10,281,11],[281,12,281,13],[282,10,282,11],[282,12,282,13],[283,10,283,11],[283,12,283,13],[284,10,284,11],[284,12,284,13],[285,10,285,11],[285,12,285,13],[286,10,286,11],[286,12,286,13],[287,10,287,11],[287,12,287,13],[288,10,288,11],[288,12,288,13],[289,0,292,3],[289,10,289,11],[289,12,289,13],[290,10,290,11],[290,12,290,13],[291,10,291,11],[291,12,291,13],[292,10,292,11],[292,12,292,13],[293,0,293,13],[294,0,294,3],[295,0,295,5],[296,0,297,0],[296,1,297,1],[296,2,297,2],[296,3,297,3],[296,4,297,4],[296,5,296,9],[296,10,297,10],[296,11,297,11],[298,0,301,3],[302,0,302,3],[303,0,308,0],[303,1,304,1],[303,2,303,6],[303,7,304,7],[309,0,309,3],[310,0,311,0],[310,1,311,1],[310,2,311,2],[310,3,311,3],[310,4,311,5],[310,6,310,8],[310,9,310,13],[310,14,311,14],[310,15,311,15],[311,6,311,7],[312,4,312,5],[312,6,312,7],[313,4,313,5],[313,6,313,7],[314,4,314,5],[314,6,314,7],[315,4,315,5],[315,6,315,7],[316,4,316,5],[316,6,316,7],[317,4,317,5],[317,6,317,7],[318,4,318,5],[318,6,318,7],[319,4,319,5],[319,6,319,7],[320,4,320,5],[320,6,320,7],[321,4,321,5],[321,6,321,7],[322,4,322,5],[322,6,322,7],[323,4,323,5],[323,6,323,7],[324,4,324,5],[324,6,324,7],[325,4,325,5],[325,6,325,7],[326,4,326,5],[326,6,326,7],[327,4,327,5],[327,6,327,7],[328,4,328,5],[328,6,328,7],[329,4,329,5],[329,6,329,7],[330,4,330,5],[330,6,330,7],[331,4,331,5],[331,6,331,7],[332,4,332,5],[332,6,332,7],[333,4,333,5],[333,6,333,7],[334,4,334,5],[334,6,334,7],[335,4,335,5],[335,6,335,7],[336,4,336,5],[336,6,336,7],[337,4,337,5],[337,6,337,7],[338,4,338,5],[338,6,338,7],[339,4,339,5],[339,6,339,7],[340,4,340,5],[340,6,340,7],[341,4,341,5],[341,6,341,7],[342,4,342,5],[342,6,342,7],[343,4,343,5],[343,6,343,7],[344,4,344,5],[344,6,344,7],[345,4,345,5],[345,6,345,7],[346,4,346,5],[346,6,346,7],[347,4,347,5],[347,6,347,7],[348,4,348,5],[348,6,348,7],[349,4,349,5],[349,6,349,7],[350,4,350,5],[350,6,350,7],[351,4,351,5],[351,6,351,7],[352,4,352,5],[352,6,352,7],[353,4,353,5],[353,6,353,7],[354,4,354,5],[354,6,354,7],[355,4,355,5],[355,6,355,7],[356,4,356,5],[356,6,356,7],[357,4,357,5],[357,6,357,7],[358,4,358,5],[358,6,358,7],[359,4,359,5],[359,6,359,7],[360,4,360,5],[360,6,360,7],[361,4,361,5],[361,6,361,7],[362,4,362,5],[362,6,362,7],[363,4,363,5],[363,6,363,7],[364,4,364,5],[364,6,364,7],[365,4,365,5],[365,6,365,7],[366,4,366,5],[366,6,366,7],[367,4,367,5],[367,6,367,7],[368,4,368,5],[368,6,368,7],[369,4,369,5],[369,6,369,7],[370,4,370,5],[370,6,370,7],[371,4,371,5],[371,6,371,7],[372,4,372,5],[372,6,372,7],[373,4,373,5],[373,6,373,7],[374,4,374,5],[374,6,374,7],[375,4,375,5],[375,6,375,7],[376,4,376,5],[376,6,376,7],[377,4,377,5],[377,6,377,7],[378,4,378,5],[378,6,378,7],[379,4,379,5],[379,6,379,7],[380,4,380,5],[380,6,380,7],[381,4,381,5],[381,6,381,7],[382,4,382,5],[382,6,382,7],[383,4,383,5],[383,6,383,7],[384,4,384,5],[384,6,384,7],[385,4,385,5],[385,6,385,7],[386,4,386,5],[386,6,386,7],[387,4,387,5],[387,6,387,7],[388,4,388,5],[388,6,388,7],[389,4,389,5],[389,6,389,7],[390,4,390,5],[390,6,390,7],[391,4,391,5],[391,6,391,7],[392,4,392,5],[392,6,392,7],[393,4,393,5],[393,6,393,7],[394,4,394,5],[394,6,394,7],[395,4,395,5],[395,6,395,7],[396,4,396,5],[396,6,396,7],[397,4,397,5],[397,6,397,7],[398,4,398,5],[398,6,398,7],[399,4,399,5],[399,6,399,7],[400,4,400,5],[400,6,400,7],[401,4,401,5],[401,6,401,7],[402,4,402,5],[402,6,402,7],[403,4,403,5],[403,6,403,7],[404,4,404,5],[404,6,404,7],[405,4,405,5],[405,6,405,7],[406,0,406,3],[407,0,412,0],[407,1,408,1],[407,2,407,6],[407,7,408,7],[413,0,413,2],[414,0,415,0],[414,1,414,5],[414,6,414,10],[414,11,414,15],[420,0,420,3],[421,0,422,0],[421,1,422,1],[421,2,421,3],[421,4,422,4],[421,5,422,5],[421,6,422,6],[421,7,421,8],[421,9,421,10],[421,11,422,11],[424,0,424,3],[425,0,426,0],[425,1,426,1],[425,2,425,3],[425,4,426,4],[425,5,426,5],[425,6,426,6],[425,7,425,13],[426,8,426,9],[426,10,426,11],[426,12,426,13],[427,0,440,0],[427,1,440,1],[427,2,440,2],[427,3,440,3],[427,4,440,4],[427,5,440,5],[427,6,440,6],[427,7,440,7],[427,8,427,9],[427,10,427,11],[427,12,427,13],[428,8,428,9],[428,10,428,11],[428,12,428,13],[429,8,429,9],[429,10,429,11],[429,12,429,13],[430,8,430,9],[430,10,430,11],[430,12,430,13],[431,8,431,9],[431,10,431,11],[431,12,431,13],[432,8,432,9],[432,10,432,11],[432,12,432,13],[433,8,433,9],[433,10,433,11],[433,12,433,13],[434,8,434,9],[434,10,434,11],[434,12,434,13],[435,8,435,9],[435,10,435,11],[435,12,435,13],[436,8,436,9],[436,10,436,11],[436,12,436,13],[437,8,437,9],[437,10,437,11],[437,12,437,13],[438,8,438,9],[438,10,438,11],[438,12,438,13],[439,8,439,9],[439,10,439,11],[439,12,439,13],[440,8,440,9],[440,10,440,11],[440,12,440,13],[441,0,441,3],[442,0,443,0],[442,1,443,1],[442,2,443,3],[442,4,442,7],[442,8,443,8],[442,9,443,9],[442,10,443,10],[442,11,443,11],[443,4,443,6],[444,2,444,3],[444,4,444,6],[445,2,445,3],[445,4,445,6],[446,2,446,3],[446,4,446,6],[447,2,447,3],[447,4,447,6],[448,2,448,3],[448,4,448,6],[449,2,449,3],[449,4,449,6],[450,2,450,3],[450,4,450,6],[451,2,451,3],[451,4,451,6],[452,2,452,3],[452,4,452,6],[453,2,453,3],[453,4,453,6],[454,2,454,3],[454,4,454,6],[455,2,455,3],[455,4,455,6],[456,2,456,3],[456,4,456,6],[457,2,457,3],[457,4,457,6],[458,0,458,3],[459,0,459,2],[460,0,461,0],[460,1,461,1],[460,2,461,2],[460,3,461,3],[460,4,460,8],[460,9,461,9],[476,0,478,2],[479,0,479,3],[480,0,481,0],[480,1,481,1],[480,2,481,2],[480,3,481,3],[480,4,480,8],[480,9,481,9],[482,0,484,2],[485,0,485,3],[486,0,490,0],[486,1,487,1],[486,2,486,6],[486,7,487,7],[493,0,493,5],[494,0,496,0],[494,1,496,1],[494,2,496,2],[494,3,496,3],[494,4,496,4],[494,5,496,7],[494,8,496,8],[494,9,496,9],[494,10,494,14],[494,15,496,15],[495,10,496,10],[495,11,496,11],[495,12,495,13],[495,14,496,14],[497,0,504,0],[497,5,497,7],[498,5,498,7],[499,5,499,7],[500,5,500,7],[501,5,501,7],[502,5,502,7],[503,5,503,7],[504,5,504,7],[505,5,505,7],[507,3,507,4],[507,5,507,6],[508,3,508,4],[508,5,508,6],[509,3,509,4],[509,5,509,6],[510,3,510,4],[510,5,510,6],[511,3,511,4],[511,5,511,6],[512,3,512,4],[512,5,512,6],[513,3,513,4],[513,5,513,6],[514,3,514,4],[514,5,514,6],[515,3,515,4],[515,5,515,6],[516,3,516,4],[516,5,516,6],[518,0,518,4],[519,0,519,4],[520,0,521,0],[520,1,521,1],[520,2,521,2],[520,3,521,3],[520,4,521,4],[520,5,520,8],[520,9,521,9],[520,10,521,10],[520,11,521,11],[520,12,521,12],[520,13,521,13],[522,0,523,0],[522,1,523,1],[566,0,567,0],[566,1,567,1],[569,0,570,0],[569,1,570,1],[629,0,630,0],[629,1,630,1],[650,0,650,4],[651,0,652,0],[651,1,652,1],[651,2,652,2],[651,3,651,6],[651,7,652,7],[651,8,652,8],[651,9,652,9],[651,10,652,10],[651,11,652,11],[651,12,652,12],[651,13,652,13],[655,0,655,6],[656,0,656,6],[657,0,657,6],[658,0,658,6],[659,0,659,6],[660,0,660,6],[661,0,661,4],[662,0,662,2]],"flags":["formulas_cached_only"]}
[]
["环境信息公开内容"]
["一、基础信息"]
["（1）排污单位基本信息"]
["排污许可证管理类别：",null,null,"重点管理"]
["单位名称：",null,null,"中孚药业股份有限公司 "]
["注册地址：",null,null,"山东省潍坊市寒亭区禹王北街2709号 "]
["生产经营场所地址：",null,null,"山东省潍坊市寒亭区禹王北街2709号 "]
["邮政编码：",null,null,"261100 "]
["行业类别：",null,null,"化学药品原料药制造 "]
["其他行业类别：",null,null,"化学药品制剂制造,锅炉"]
["是否投产：",null,null,"是"]
["投产日期：",null,null,"2011-01-03 "]
["生产经营场所中心经度：",null,null,"119  度 10  分 13.15  秒"]
["生产经营场所中心纬度：",null,null,"36  度 47  分 20.94  秒"]
["组织机构代码："]
["统一社会信用代码：",null,null,"913707037232674976 "]
["法定代表人（主要负责人）：",null,null,"姜林海 "]
["技术负责人：",null,null,"王殿勇 "]
["固定电话：",null,null,"0536-2206836 "]
["移动电话：",null,null,"13791686128 "]
["（2）主要产品及产能"]
["行业类别","主要生产单元名称","主要工艺名称","生产设施名称","生产设施编号","设施参数",{"$nulls":3},"产品名称","计量单位","生产能力","近三年实际产量（t/a）","设计年生产时间（h）","其他产品信息","其他工艺信息"]
[{"$nulls":5},"参数名称","计量单位","设计值","其他设施参数信息"]
["化学药品原料药制造","卡托普利生产线","反应","不锈钢反应罐","MF0041","容积","L",2000,null,"卡托普利","t",300,188,7200]
[{"$nulls":3},"搪玻璃反应罐","MF0040","容积","L",2000,"缩合罐,功率5.5KW"]
[{"$nulls":3},"搪玻璃反应罐","MF0042","容积","L",1500,"缩合罐，功率5.5KW"]
[{"$nulls":3},"搪玻璃反应罐","MF0053","容积","L",1500,"缩合罐，功率5.5KW"]
[{"$nulls":3},"搪玻璃反应罐","MF0054","容积","L",1500,"缩合罐，功率5.5KW"]
[{"$nulls":3},"搪玻璃反应罐","MF0055","容积","L",1500,"中和罐，功率4.0KW"]
[{"$nulls":3},"搪玻璃反应罐","MF0056","容积","L",1500,"中和罐，功率4.0KW"]
[{"$nulls":3},"搪玻璃反应罐","MF0057","容积","L",1500,"中和罐，功率4.0KW"]
[{"$nulls":3},"搪玻璃反应罐","MF0058","容积","L",1500,"中和罐，功率4.0KW"]
[null,"卡托普利生产线","水解","搪玻璃反应罐","MF0044","容积","L",1000,"水解罐"]
[{"$nulls":3},"搪玻璃反应罐","MF0045","容积","L",1000,"水解罐"]
[null,"卡托普利生产线","干燥","回收卡托普利干燥器","MF0060","容积","L",1000,"功率：4KW"]
[{"$nulls":3},"双锥回转真空干燥机","MF0047","容积","t",1,"容积1000L，功率4KW"]
[{"$nulls":3},"双锥回转真空干燥机","MF0059","容积","t",1,"容积1000L，功率4KW"]
[null,"卡托普利生产线","配料","碱液计量罐","MF0066","容积","L",500]
[{"$nulls":3},"碱液计量罐","MF0067","容积","L",500]
[{"$nulls":3},"碱液计量罐","MF0068","容积","L",500]
[{"$nulls":3},"碱液计量罐","MF0069","容积","L",500]
[{"$nulls":3},"母液回收罐","MF0082","容积","L",2000]
[{"$nulls":3},"母液回收罐","MF0083","容积","L",2000]
[{"$nulls":3},"浓盐酸计量罐","MF0084","容积","L",300]
[{"$nulls":3},"浓盐酸计量罐","MF0085","容积","L",300]
[{"$nulls":3},"浓盐酸计量罐","MF0086","容积","L",300]
[{"$nulls":3},"浓盐酸计量罐","MF0087","容积","L",300]
[{"$nulls":3},"配碱罐","MF0063","容积","L",1500,"功率：4.0KW"]
[{"$nulls":3},"配碱罐","MF0064","容积","L",500,"功率：3.0KW"]
[{"$nulls":3},"双氧水计量罐","MF0080","容积","L",200]
[{"$nulls":3},"双氧水计量罐","MF0081","容积","L",200]
[{"$nulls":3},"水计量罐","MF0061","容积","L",800,"配碱"]
[{"$nulls":3},"水计量罐","MF0062","容积","L",500,"配碱"]
[{"$nulls":3},"水计量罐","MF0065","容积","L",800,"配料"]
[{"$nulls":3},"水计量罐","MF0079","容积","L",800,"用途：洗涤"]
[{"$nulls":3},"酰氯计量罐","MF0070","容积","L",200]
[{"$nulls":3},"酰氯计量罐","MF0071","容积","L",200]
[{"$nulls":3},"酰氯计量罐","MF0072","容积","L",200]
[{"$nulls":3},"酰氯计量罐","MF0073","容积","L",200]
[{"$nulls":3},"盐酸计量罐","MF0074","容积","L",300]
[{"$nulls":3},"盐酸计量罐","MF0075","容积","L",300]
[{"$nulls":3},"盐酸计量罐","MF0076","容积","L",300]
[{"$nulls":3},"盐酸计量罐","MF0077","容积","L",300]
[{"$nulls":3},"盐酸计量罐","MF0078","容积","L",300]
[null,"卡托普利生产线","分离","过滤打料泵","MF0089","功率","KW",3,"CQ50-32-125"]
[{"$nulls":3},"过滤打料泵","MF0090","功率","KW",3,"CQ50-32-125"]
[{"$nulls":3},"过滤打料泵","MF0091","功率","KW",3,"CQ50-32-125"]
[{"$nulls":3},"过滤打料泵","MF0092","功率","KW",3,"CQ50-32-125"]
[{"$nulls":3},"过滤打料泵","MF0093","功率","KW",3,"CQ50-32-125"]
[{"$nulls":3},"离心机","MF0046","容积","L",1000,"功率：11KW"]
[{"$nulls":3},"离心机","MF0088","容积","L",1000,"功率：11KW"]
[{"$nulls":3},"离心机","MF0099","额定功率","kw",22,"型号：LGZ-1250"]
[{"$nulls":3},"离心机","MF0100","额定功率","kw",22,"型号：LGZ-1250"]
[{"$nulls":3},"离心机","MF0101","额定功率","kw",22,"型号：LGZ-1250"]
[{"$nulls":3},"离心机","MF0102","额定功率","kw",22,"型号：LGZ-1250"]
[{"$nulls":3},"离心机","MF0103","额定功率","kw",55,"型号：GKC-1250"]
[{"$nulls":3},"离心机","MF0104","额定功率","kw",55,"型号：GKC-1250"]
[{"$nulls":3},"钛棒过滤器","MF0094","容积","L",1000]
[{"$nulls":3},"钛棒过滤器","MF0095","容积","L",1000]
[{"$nulls":3},"钛棒过滤器","MF0096","容积","L",1000]
[{"$nulls":3},"钛棒过滤器","MF0097","容积","L",1000]
[{"$nulls":3},"钛棒过滤器","MF0098","容积","L",1000]
[null,"卡托普利生产线","精制","结晶罐","MF0105","容积","L",1500,"功率：4KW",{"$nulls":6},"与酸化工序二合一设备"]
[{"$nulls":3},"结晶罐","MF0106","容积","L",1500,"功率：4KW"]
[{"$nulls":3},"结晶罐","MF0107","容积","L",1500,"功率：4KW"]
[null,"卡托普利生产线","成品","混粉机","MF0048","额定功率","kw",5.5,"YYH-4000,一维混合器"]
[{"$nulls":3},"磨粉机","MF0109","额定功率","kw",11.55,"型号:40B-X"]
[{"$nulls":3},"振荡筛","MF0108","额定功率","kw",1.5,"型号：ZS-1000"]
["化学药品原料药制造","乙酰谷酰氨生产线","反应","反应接受罐","MF0037","容积","L",300,null,"乙酰谷酰氨","t",63.3,30,7200,"该生产线其它品种：盐酸肼曲嗪0……"]
[{"$nulls":3},"反应接受罐","MF0162","容积","L",300]
[{"$nulls":3},"反应冷凝器","MF0163","面积","m2",20]
[{"$nulls":3},"离心母液槽","MF0160","容积","L",216]
[{"$nulls":3},"离心母液槽","MF0161","容积","L",216]
[{"$nulls":3},"搪玻璃反应罐","MF0035","容积","L",1000]
[{"$nulls":3},"脱色槽","MF0164","容积","L",1500,"功率：4kw"]
[{"$nulls":3},"中转槽","MF0165","容积","L",1500,"功率：4KW"]
[null,"乙酰谷酰氨生产线","分离","过滤打料泵","MF0167","功率","KW",3,"CQ50-32-125"]
[{"$nulls":3},"过滤打料泵","MF0168","功率","KW",3,"CQ50-32-125"]
[{"$nulls":3},"三足式人工上卸料离心机","MF0038","功率","KW",18.5,"型号：LB-1250"]
[{"$nulls":3},"三足式人工上卸料离心机","MF0166","功率","KW",18.5,"型号：LB-1000"]
[{"$nulls":3},"钛棒过滤器","MF0169","面积","m2",20]
[{"$nulls":3},"钛棒过滤器","MF0170","面积","m2",20]
[null,"乙酰谷酰氨生产线","干燥","热水泵","MF0172","额定功率","kw",15,"型号：IH100"]
[{"$nulls":3},"热水泵","MF0173","额定功率","kw",15,"型号：IH100"]
[{"$nulls":3},"热水罐","MF0171","容积","L",5000]
[{"$nulls":3},"双锥干燥器","MF0039","容积","L",500]
[null,"乙酰谷酰胺生产线","配料","甲醇溶解罐","MF0174","容积","L",300,"功率：2.2KW"]
[{"$nulls":3},"异丙醇计量罐","MF0175","容积","L",200]
[null,"乙酰谷酰胺生产线","精制","结晶罐","MF0176","容积","L",500,"功率：4KW",{"$nulls":6},"与酸化工序二合一设备"]
[{"$nulls":3},"结晶罐","MF0177","容积","L",500,"功率：4KW"]
[{"$nulls":3},"结晶罐","MF0178","容积","L",500,"功率：4KW"]
[null,"乙酰谷酰胺生产线","成品","混粉机","MF0181","额定功率","kw",4,"型号：YYH-4000"]
[{"$nulls":3},"磨粉机","MF0179","额定功率","kw",11.55,"型号：40B-X"]
[{"$nulls":3},"振荡筛","MF0180","额定功率","kw",1.5,"型号：ZS-1000"]
[null,"乙酰谷酰胺生产线","溶剂回收","回收罐","MF0184","容积","L",500]
[{"$nulls":3},"冷凝器","MF0183","面积","m2",10]
[{"$nulls":3},"蒸馏罐","MF0182","容积","L",1500,"功率：4KW"]
["化学药品原料药制造","公用单元","污水处理设施","二沉池","MF0193","规格","mm","--","5500×7000×7000m……"]
[{"$nulls":3},"混凝沉淀池","MF0049","容积","m3",1000]
[{"$nulls":3},"曝气生物滤池","MF0050","容积","m3",1000]
[{"$nulls":3},"水解酸化池","MF0192","容积","mm","--","9550×7500×7000m……"]
[{"$nulls":3},"中和池","MF0051","容积","m3",500]
[null,"公用单元","固废处理处置系统","危险废物暂存间","MF0194","面积","m2",100]
[null,"公用单元","纯水制备系统","保安过滤装置","MF0205","其他","--","--","5芯"]
[{"$nulls":3},"保安过滤装置","MF0206","其他","--","--","5芯"]
[{"$nulls":3},"保安过滤装置","MF0207","其他","--","--","5芯"]
[{"$nulls":3},"保安过滤装置","MF0208","其他","--","--","5芯"]
[{"$nulls":3},"保安过滤装置","MF0209","其他","--","--","5芯"]
[{"$nulls":3},"纯水储罐","MF0215","容积","t",5]
[{"$nulls":3},"纯水储罐","MF0216","容积","t",5]
[{"$nulls":3},"纯水储罐","MF0217","容积","t",5]
[{"$nulls":3},"纯水储罐","MF0218","容积","t",5]
[{"$nulls":3},"纯水储罐","MF0219","容积","t",5]
[{"$nulls":3},"反渗透装置","MF0210","流量","m3/h",3.6,"二级反渗透，型号：HDRO-S……"]
[{"$nulls":3},"反渗透装置","MF0211","流量","m3/h",3.6,"二级反渗透，型号：HDRO-S……"]
[{"$nulls":3},"反渗透装置","MF0212","流量","m3/h",3.6,"二级反渗透，型号：HDRO-S……"]
[{"$nulls":3},"反渗透装置","MF0213","流量","m3/h",3.6,"二级反渗透，型号：HDRO-S……"]
[{"$nulls":3},"反渗透装置","MF0214","流量","m3/h",3.6,"二级反渗透，型号：HDRO-S……"]
[{"$nulls":3},"活性炭吸附装置","MF0195","处理量","t/h",5,"型号：HQ600"]
[{"$nulls":3},"活性炭吸附装置","MF0196","处理量","t/h",5,"型号：HQ600"]
[{"$nulls":3},"活性炭吸附装置","MF0197","处理量","t/h",5,"型号：HQ600"]
[{"$nulls":3},"活性炭吸附装置","MF0198","处理量","t/h",5,"型号：HQ600"]
[{"$nulls":3},"活性炭吸附装置","MF0199","处理量","t/h",5,"型号：HQ600"]
[{"$nulls":3},"砂滤装置","MF0200","容积","m3",5,"型号：JQ600"]
[{"$nulls":3},"砂滤装置","MF0201","容积","m3",5,"型号：JQ600"]
[{"$nulls":3},"砂滤装置","MF0202","容积","m3",5,"型号：JQ600"]
[{"$nulls":3},"砂滤装置","MF0203","容积","m3",5,"型号：JQ600"]
[{"$nulls":3},"砂滤装置","MF0204","容积","m3",5,"型号：JQ600"]
[null,"公用单元","事故应急系统","围堰","MF0221","容积","m3",20]
[{"$nulls":3},"围堰","MF0222","容积","m3",45]
[{"$nulls":3},"消防废水池","MF0223","容积","m3",600]
[{"$nulls":3},"应急事故池","MF0220","容积","m3",100]
[null,"公用单元","物料存储系统","常压罐","MF0226","容积","m3",10,"内盛盐酸"]
[{"$nulls":3},"常压罐","MF0227","容积","m3",10,"内盛盐酸"]
[{"$nulls":3},"常压罐","MF0228","容积","m3",20,"内盛盐酸"]
[{"$nulls":3},"成品库房","MF0225","面积","m2",2028.25]
[{"$nulls":3},"化学品库","MF0224","面积","m2",905.85]
[null,"卡托普利生产线","废气处理系统","布袋除尘器","MF0229","处理能力","m3/h",10000]
[{"$nulls":3},"吸收塔","MF0230","处理能力","m3/h",10000]
[null,"乙酰谷酰胺生产线","废气处理系统","3级碱洗+1级水喷淋处理设施","MF0231","处理能力","m3/h",10000]
[null,"公用单元","废气处理系统","喷淋洗涤塔+复合催化氧化装置+活性炭吸附装置","MF0232","处理能力","m3/h",5000]
[]
["行业类别","生产线名称","生产线编号","产品类别","产品名称","产品规格",null,"产品数量",null,"生产能力（t/a）","设计年运行时间（h）","其他产品信息"]
[{"$nulls":5},"数量","计量单位","数量","计量单位"]
["化学药品制剂制造","液体制剂生产线","水针剂生产线","水针剂","硫酸庆大霉素注射液",1,"ml/支",100000000,"支/a",5000,7200,"该生产线其他品种：阿魏酸钠注射……"]
["化学药品制剂制造","固体制剂生产线","固体制剂生产线","片剂","含有生物碱及其衍生物片剂",10,"mg/片",1500000000,"片/a",5,7200,"卡托普利片剂，该生产线其他品种……"]
[{"$nulls":3},"粉针剂","含有青霉素及其衍生物粉针剂",5,"ml/瓶",150000000,"支/a",5,7200,"美洛西林钠针剂，该生产线其他生……"]
["化学药品制剂制造","液体制剂生产线","口服液生产线","口服液","普瑞巴林口服溶液",10,"ml/瓶",10000000,"瓶/a",9.6,2400,"巴氯芬口服溶液200万瓶，其他……"]
[]
["行业类别","生产线名称","生产线编号","主要生产单元名称","主要工艺名称","生产设施名称","生产设施编号","设施参数",{"$nulls":3},"其他设施信息","其他工艺信息"]
[{"$nulls":7},"参数名称","计量单位","设计值","其他设施参数信息"]
["化学药品制剂制造","液体制剂生产线","水针剂生产线","注射液","清洗","超声波清洗机","MF0185","清洗能力","支/h",25000,null,"清洗2ml瓶，25000支/h……"]
[{"$nulls":5},"立式超声波清洗机","MF0186","清洗能力","支/h",12000,"清洗10ml瓶，12000支/……"]
[{"$nulls":3},"注射液","配料","不锈钢配料罐","MF0187","生产能力","L",500,null,null,"该设备同时为原料过滤设备。"]
[{"$nulls":5},"不锈钢配料罐","MF0188","生产能力","L",1500]
[{"$nulls":3},"注射液","烘干","干燥灭菌器","MF0189","处理能力","支/h",25000,"处理2ml瓶，25000支/h……"]
[{"$nulls":3},"注射液","灌装","灌装封口机","MF0191","处理能力","支/h",12000,"处理10ml瓶，12000支/……"]
[{"$nulls":5},"罐装封口机","MF0190","处理能力","支/h",25000,"处理2ml瓶，25000支/h……"]
["化学药品制剂制造","固体制剂生产线","固体制剂生产线","片剂","干燥","沸腾床","MF0110","生产能力","kg/锅",120,"FG-60"]
[{"$nulls":5},"热风循环烘箱","MF0111","容积","kg/锅",120,"SH-I"]
[{"$nulls":5},"热风循环烘箱","MF0112","容积","kg/锅",120,"SH-I"]
[{"$nulls":5},"热风循环烘箱","MF0113","容积","kg/锅",120,"SH-I"]
[{"$nulls":5},"热风循环烘箱","MF0114","容积","kg/锅",120,"SH-I"]
[{"$nulls":5},"热风循环烘箱","MF0115","容积","kg/锅",120,"SH-I"]
[{"$nulls":5},"热风循环烘箱","MF0116","容积","kg/锅",120,"SH-I"]
[{"$nulls":5},"热风循环烘箱","MF0117","容积","kg/锅",120,"SH-I"]
[{"$nulls":5},"热风循环烘箱","MF0118","容积","kg/锅",120,"SH-I"]
[{"$nulls":5},"热风循环烘箱","MF0119","容积","kg/锅",120,"SH-I"]
[{"$nulls":5},"热风循环烘箱","MF0120","容积","kg/锅",120,"SH-I"]
[{"$nulls":5},"热风循环烘箱","MF0121","容积","kg/锅",120,"SH-I"]
[{"$nulls":3},"片剂","粉碎","不锈钢粉碎机","MF0122","生产能力","kg/h",300]
[{"$nulls":3},"胶囊剂","分装","全自动硬胶囊填充机","MF0123","装载量","万粒/h",15]
[{"$nulls":3},"片剂","混合","三维运动混合机","MF0124","处理量","kg/锅",60]
[{"$nulls":5},"三维运动混合机","MF0125","处理量","kg/锅",60]
[{"$nulls":3},"颗粒剂","制粒","高速混合制粒机","MF0137","处理量","kg/锅",10]
[{"$nulls":5},"高效湿法混合制粒机","MF0136","处理量","kg/锅",120]
[{"$nulls":5},"振荡筛","MF0126","处理量","kg/h",300]
[{"$nulls":5},"振荡筛","MF0127","处理量","kg/h",300]
[{"$nulls":5},"振荡筛","MF0128","处理量","kg/h",300]
[{"$nulls":5},"振荡筛","MF0129","处理量","kg/h",300]
[{"$nulls":5},"振荡筛","MF0130","处理量","kg/h",300]
[{"$nulls":5},"振荡筛","MF0131","处理量","kg/h",300]
[{"$nulls":5},"整粒机","MF0132","处理量","kg/锅",60]
[{"$nulls":5},"整粒机","MF0133","处理量","kg/锅",60]
[{"$nulls":5},"整粒机","MF0134","处理量","kg/锅",60]
[{"$nulls":5},"整粒机","MF0135","处理量","kg/锅",60]
[{"$nulls":3},"片剂","压片","全自动高速压片机","MF0138","生产能力","万片/h",38.2]
[{"$nulls":3},"片剂","包衣","包衣机","MF0139","生产能力","kg/锅",40]
[{"$nulls":5},"包衣机","MF0140","生产量","kg/锅",20]
[{"$nulls":5},"包衣机","MF0141","生产量","kg/锅",20]
[{"$nulls":5},"包衣机","MF0142","生产量","kg/锅",20]
[{"$nulls":3},"粉针剂","清洗","超声波清洗机","MF0143","处理能力","瓶/h",23000,"处理7ml瓶，23000瓶/h……"]
[{"$nulls":5},"超声波清洗机","MF0144","处理能力","瓶/h",23000,"处理7ml瓶，23000瓶/h……"]
[{"$nulls":5},"超声波清洗机","MF0145","处理能力","瓶/h",23000,"处理7ml瓶，23000瓶/h……"]
[{"$nulls":5},"超声波清洗机","MF0146","处理能力","瓶/h",23000,"处理7ml瓶，23000瓶/h……"]
[{"$nulls":3},"粉针剂","混合","一维运动混合机","MF0147","处理能力","kg/锅",600,"规格型号：YYH-600"]
[{"$nulls":5},"一维运动混合机","MF0148","处理能力","kg/锅",600,"规格型号：YYH-600"]
[{"$nulls":5},"一维运动混合机","MF0149","处理能力","kg/锅",600,"规格型号：YYH-600"]
[{"$nulls":5},"一维运动混合机","MF0150","处理能力","kg/锅",600,"规格型号：YYH-600"]
[{"$nulls":3},"粉针剂","干燥","不锈钢恒温烘箱","MF0153","容积","L",50]
[{"$nulls":5},"电热恒温鼓风干燥箱","MF0155","容积","L",50]
[{"$nulls":5},"二合一装置","MF0151","生产能力","瓶/h",23000,"处理7ml瓶，23000瓶/h……","隧道式灭菌干燥机,规格型号：G……"]
[{"$nulls":5},"二合一装置","MF0152","容积","L",2000,"电热灭菌烘箱"]
[{"$nulls":5},"旋转除湿器","MF0154","--","--","--","规格型号：ZL-20Q-L"]
[{"$nulls":3},"粉针剂","分装","分装机","MF0156","处理量","瓶/h",23000,"处理7ml瓶，23000瓶/h……"]
[{"$nulls":5},"分装机","MF0157","处理量","瓶/h",23000,"处理7ml瓶，23000瓶/h……"]
[{"$nulls":5},"分装机","MF0158","处理量","瓶/h",23000,"处理7ml瓶，23000瓶/h……"]
[{"$nulls":5},"分装机","MF0159","处理量","瓶/h",23000,"处理7ml瓶，23000瓶/h……"]
["化学药品制剂制造","液体制剂生产线","口服液生产线","口服液","配置","配制罐","MF0233","容积","L",200]
[{"$nulls":5},"配制罐","MF0234","容积","L",3000]
[{"$nulls":3},"口服液","过滤","过滤器","MF0235","处理量","L/h",10000]
[{"$nulls":3},"口服液","滤液储罐","滤液储罐","MF0236","容积","L",2000]
[{"$nulls":3},"口服液","灌装","罐装联动线","MF0237","生产能力","瓶/分",60]
[{"$nulls":3},"口服液","清洗","包装联动线","MF0238","生产能力","瓶/分",60]
["二、排污信息"]
["1、排放口"]
["（1）大气排放口基本情况表"]
["排放口编号","排放口名称","污染物种类",null,null,"排放口地理坐标",null,"排气筒高度（m）","排气筒出口内径","排气温度","其他信息"]
[{"$nulls":5},"经度","纬度",null,"（m）"]
["DA001","废气排放口","挥发性有机物,总挥发性有机物,颗粒物,氯化氢,甲醇,异丙醇,二氯甲烷,乙醇,四氢呋喃,乙酸乙酯,丙酮,正己烷,甲酸乙酯,氯乙酸乙酯,三氯甲烷",null,null,"119度 10分 13.15秒","36度 47分 20.94秒",15,0.3,"常温"]
["DA003","污水处理设施废气排放口","挥发性有机物,臭气浓度,氨（氨气）,硫化氢,苯系物",null,null,"119度 10分 4.30秒","36度 47分 25.15秒",15,0.3,"常温"]
["（2）废气污染物排放执行标准信息表"]
["排放口编号","排放口名称","污染物种类","国家或地方污染物排放标准",{"$nulls":5},"环境影响评价批复要求","承诺更加严格排放限值",null,"其他信息"]
[{"$nulls":3},"名称",{"$nulls":3},"浓度限值","速率限值（kg/h）"]
["DA001","废气排放口","乙酸乙酯","/",{"$nulls":3},"/mg/Nm3","/","/ mg/Nm3","/ mg/Nm3"]
["DA001","废气排放口","颗粒物","山东省区域性大气污染物综合排放标准DB37/2376-2013",{"$nulls":3},"10mg/Nm3","/","/ mg/Nm3","/ mg/Nm3",null,"/"]
["DA001","废气排放口","甲酸乙酯","/",{"$nulls":3},"/mg/Nm3","/","/ mg/Nm3","/ mg/Nm3"]
["DA001","废气排放口","乙醇","/",{"$nulls":3},"/mg/Nm3","/","/ mg/Nm3","/ mg/Nm3"]
["DA001","废气排放口","总挥发性有机物","制药工业大气污染物排放标准GB37823—2019",{"$nulls":3},"100mg/Nm3","/","/ mg/Nm3","/ mg/Nm3",null,"/"]
["DA001","废气排放口","异丙醇","/",{"$nulls":3},"/mg/Nm3","/","/ mg/Nm3","/ mg/Nm3"]
["DA001","废气排放口","丙酮","挥发性有机物排放标准 第6部分：有机化工行业DB37/2801.6-2018",{"$nulls":3},"50mg/Nm3","/","/ mg/Nm3","/ mg/Nm3"]
["DA001","废气排放口","三氯甲烷","挥发性有机物排放标准 第6部分：有机化工行业DB37/2801.6-2018",{"$nulls":3},"50mg/Nm3","/","/ mg/Nm3","/ mg/Nm3"]
["DA001","废气排放口","正己烷","挥发性有机物排放标准 第6部分：有机化工行业DB37/2801.6-2018",{"$nulls":3},"50mg/Nm3","/","/ mg/Nm3","/ mg/Nm3"]
["DA001","废气排放口","甲醇","挥发性有机物排放标准 第6部分：有机化工行业DB37/2801.6-2018",{"$nulls":3},"50mg/Nm3","/","/ mg/Nm3","/ mg/Nm3"]
["DA001","废气排放口","氯乙酸乙酯","/",{"$nulls":3},"/mg/Nm3","/","/ mg/Nm3","/ mg/Nm3"]
["DA001","废气排放口","挥发性有机物","挥发性有机物排放标准第6部分：有机化工行业DB37/2801.6-2018",{"$nulls":3},"60mg/Nm3",3,"/ mg/Nm3","/ mg/Nm3",null,"污染治理设施处理效率达到90%及以上时，不执行排放速率限值要求"]
["DA001","废气排放口","四氢呋喃","挥发性有机物排放标准 第6部分：有机化工行业DB37/2801.6-2018",{"$nulls":3},"50mg/Nm3","/","/ mg/Nm3","/ mg/Nm3"]
["DA001","废气排放口","氯化氢","制药工业大气污染物排放标准GB37823—2019",{"$nulls":3},"30mg/Nm3","/","/ mg/Nm3","/ mg/Nm3",null,"/"]
["DA001","废气排放口","二氯甲烷","挥发性有机物排放标准 第6部分：有机化工行业DB37/2801.6-2018",{"$nulls":3},"50mg/Nm3","/","/ mg/Nm3","/ mg/Nm3"]
["DA003","污水处理设施废气排放口","硫化氢","有机化工企业污水处理厂（站）挥发性有机物及恶臭污染物排放标准DB37/3161-2018",{"$nulls":3},"3mg/Nm3",0.1,"/ mg/Nm3","/ mg/Nm3",null,"环评批复标准限值为0.33kg/h."]
["DA003","污水处理设施废气排放口","氨（氨气）","有机化工企业污水处理厂（站）挥发性有机物及恶臭污染物排放标准DB37/3161-2018",{"$nulls":3},"20mg/Nm3",1,"/ mg/Nm3","/ mg/Nm3",null,"环评批复标准限值为4.9kg/h"]
["DA003","污水处理设施废气排放口","臭气浓度","有机化工企业污水处理厂（站）挥发性有机物及恶臭污染物排放标准DB37/3161-2018",{"$nulls":3},800,"/",2000,"/"]
["DA003","污水处理设施废气排放口","挥发性有机物","制药工业大气污染物排放标准GB37823—2019",{"$nulls":3},"60mg/Nm3","/","/ mg/Nm3","/ mg/Nm3"]
["DA003","污水处理设施废气排放口","苯系物","有机化工企业污水处理厂（站）挥发性有机物及恶臭污染物排放标准DB37/3161-2018",{"$nulls":3},"10mg/Nm3",1.6,"/ mg/Nm3","/ mg/Nm3"]
["2、大气污染物有组织排放信息"]
["  （1）主要排放口"]
["排放口编号","排放口名称","污染物种类","申请许可排放浓度限值","申请许可排放速率限值(kg/h)","申请年许可排放量限值（t/a）",{"$nulls":4},"申请特殊排放浓度限值",null,"申请特殊时段许可排放量限值"]
[{"$nulls":5},"第一年","第二年","第三年","第四年","第五年"]
["DA001","废气排放口","正己烷","50mg/Nm3","/","/","/","/","/","/","/mg/Nm3",null,"/"]
["DA001","废气排放口","二氯甲烷","50mg/Nm3","/","/","/","/","/","/","/mg/Nm3",null,"/"]
["DA001","废气排放口","丙酮","50mg/Nm3","/","/","/","/","/","/","/mg/Nm3",null,"/"]
["DA001","废气排放口","颗粒物","10mg/Nm3","/","/","/","/","/","/","/mg/Nm3",null,"/"]
["DA001","废气排放口","挥发性有机物","60mg/Nm3",3,5.184,5.184,5.184,5.184,5.184,"/mg/Nm3",null,"/"]
["DA001","废气排放口","三氯甲烷","50mg/Nm3","/","/","/","/","/","/","/mg/Nm3",null,"/"]
["DA001","废气排放口","氯乙酸乙酯","/mg/Nm3","/","/","/","/","/","/","/mg/Nm3",null,"/"]
["DA001","废气排放口","乙醇","/mg/Nm3","/","/","/","/","/","/","/mg/Nm3",null,"/"]
["DA001","废气排放口","四氢呋喃","50mg/Nm3","/","/","/","/","/","/","/mg/Nm3",null,"/"]
["DA001","废气排放口","总挥发性有机物","100mg/Nm3","/","/","/","/","/","/","/mg/Nm3",null,"/"]
["DA001","废气排放口","氯化氢","30mg/Nm3","/","/","/","/","/","/","/mg/Nm3",null,"/"]
["DA001","废气排放口","甲酸乙酯","/mg/Nm3","/","/","/","/","/","/","/mg/Nm3",null,"/"]
["DA001","废气排放口","乙酸乙酯","/mg/Nm3","/","/","/","/","/","/","/mg/Nm3",null,"/"]
["DA001","废气排放口","异丙醇","/mg/Nm3","/","/","/","/","/","/","/mg/Nm3",null,"/"]
["DA001","废气排放口","甲醇","50mg/Nm3","/","/","/","/","/","/","/mg/Nm3",null,"/"]
["DA003","污水处理设施废气排放口","挥发性有机物","60mg/Nm3","/",0.72,0.72,0.72,0.72,0.72,"/mg/Nm3",null,"/"]
["DA003","污水处理设施废气排放口","臭气浓度",800,"/","/","/","/","/","/","/mg/Nm3",null,"/"]
["DA003","污水处理设施废气排放口","氨（氨气）","20mg/Nm3",1,"/","/","/","/","/","/mg/Nm3",null,"/"]
["DA003","污水处理设施废气排放口","苯系物","10mg/Nm3",1.6,"/","/","/","/","/","/mg/Nm3",null,"/"]
["DA003","污水处理设施废气排放口","硫化氢","3mg/Nm3",0.1,"/","/","/","/","/","/mg/Nm3",null,"/"]
["主要排放口合计",{"$nulls":3},"颗粒物","/","/","/","/","/","/",null,"/ "]
[{"$nulls":4},"SO2","/","/","/","/","/","/",null,"/ "]
[{"$nulls":4},"NOx","/","/","/","/","/","/",null,"/ "]
[{"$nulls":4},"VOCs",5.904,5.904,5.904,5.904,5.904,"/",null,"/ "]
["我公司执行潍坊市寒亭区重污染天气应急预案，并严格落实。"]
[" （2）一般排放口"]
["说明：浓度限值未显示单位的，默认单位为“mg/Nm³”。"]
["排放口编号","排放口名称","污染物种类","申请许可排放浓度限值","申请许可排放速率限值(kg/h)","申请年许可排放量限值（t/a）",{"$nulls":4},"申请特殊排放浓度限值","申请特殊时段许可排放量限值"]
[{"$nulls":5},"第一年","第二年","第三年","第四年","第五年"]
["一般排放口合计",{"$nulls":3},"颗粒物","/ ","/ ","/ ","/ ","/ ","/","/ "]
[{"$nulls":4},"SO2","/ ","/ ","/ ","/ ","/ ","/","/ "]
[{"$nulls":4},"NOx","/ ","/ ","/ ","/ ","/ ","/","/ "]
[{"$nulls":4},"VOCs","/ ","/ ","/ ","/ ","/ ","/","/ "]
[" （3）全厂有组织排放总计"]
["全厂有组织排放总计","污染物种类","申请年许可排放量限值（t/a）",{"$nulls":4},"申请特殊时段许可排放量限值"]
[null,null,"第一年","第二年","第三年","第四年","第五年"]
[null,"颗粒物","/","/","/","/","/","/ "]
[null,"SO2","/","/","/","/","/","/ "]
[null,"NOx","/","/","/","/","/","/ "]
[null,"VOCs",5.904,5.904,5.904,5.904,5.904,"/ "]
["3、大气污染物无组织排放信息"]
["行业","生产设施编号/无组织排放编号","产污环节","污染物种类","主要污染防治措施",null,"国家或地方污染物排放标准",null,null,"年许可排放量限值（t/a）",{"$nulls":4},"申请特殊时段许可排放量限值","其他信息"]
[{"$nulls":6},"名称",null,"浓度限值","第一年","第二年","第三年","第四年","第五年"]
["化学药品原料药制造","厂界",null,"氨（氨气）","无组织排放控制措施",null,"有机化工企业污水处理厂（站）挥发性有机物及恶臭污染物排放标准DB37/3161-2018",null,"1.0mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","厂界",null,"苯系物","无组织排放控制措施",null,"有机化工企业污水处理厂（站）挥发性有机物及恶臭污染物排放标准DB37/3161-2018",null,"1.0mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","厂界",null,"丙酮","密闭配套有效的管网送至净化系统,密闭并配备有效的废气捕集装置（如局部密闭罩、整体密闭罩、大容积密闭罩等）",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","厂界",null,"臭气浓度","无组织排放控制措施",null,"有机化工企业污水处理厂（站）挥发性有机物及恶臭污染物排放标准DB37/3161-2018",null,"20无量纲","/","/","/","/","/","/"]
["化学药品原料药制造","厂界",null,"二氯甲烷","密闭并配备有效的废气捕集装置（如局部密闭罩、整体密闭罩、大容积密闭罩等）",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","厂界",null,"挥发性有机物","无组织排放控制措施",null,"挥发性有机物排放标准第6部分：有机化工行业DB37/2801.6-2018",null,"2.0mg/Nm3","/","/","/","/","/","/","污染治理设施处理效率达到90%……"]
["化学药品原料药制造","厂界",null,"颗粒物","无组织排放控制措施",null,"大气污染物综合排放标准GB16297-1996",null,"1.0mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","厂界",null,"甲醇","密闭配套有效的管网送至净化系统,密闭并配备有效的废气捕集装置（如局部密闭罩、整体密闭罩、大容积密闭罩等）",null,"大气污染物综合排放标准GB 16297-1996",null,"12mg/Nm3","/","/","/","/","/","/","周界外浓度最高点"]
["化学药品原料药制造","厂界",null,"氯化氢","无组织废气控制措施",null,"制药工业大气污染物排放标准GB37823—2019",null,"0.20mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","厂界",null,"四氢呋喃","密闭配套有效的管网送至净化系统,密闭并配备有效的废气捕集装置（如局部密闭罩、整体密闭罩、大容积密闭罩等）",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","厂界",null,"乙醇","密闭配套有效的管网送至净化系统,密闭并配备有效的废气捕集装置（如局部密闭罩、整体密闭罩、大容积密闭罩等）",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","厂界",null,"乙酸乙酯","密闭配套有效的管网送至净化系统,密闭并配备有效的废气捕集装置（如局部密闭罩、整体密闭罩、大容积密闭罩等）",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","厂界",null,"正己烷","密闭配套有效的管网送至净化系统,密闭并配备有效的废气捕集装置（如局部密闭罩、整体密闭罩、大容积密闭罩等）",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","厂界",null,"硫化氢","无组织排放控制措施",null,"有机化工企业污水处理厂（站）挥发性有机物及恶臭污染物排放标准DB37/3161-2018",null,"0.03mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0044","反应","颗粒物",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0042","反应","颗粒物",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0041","反应","颗粒物",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0044","反应","挥发性有机物",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0045","反应","挥发性有机物",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0041","反应","挥发性有机物",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0042","反应","挥发性有机物",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0045","反应","颗粒物",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0050","废水处理","挥发性有机物",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0051","废水处理","挥发性有机物",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0051","废水处理","臭气浓度",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0050","废水处理","臭气浓度",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0049","废水处理","臭气浓度",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0051","废水处理","氨（氨气）",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0050","废水处理","氨（氨气）",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0049","废水处理","氨（氨气）",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0049","废水处理","挥发性有机物",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0051","废水处理","硫化氢",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0050","废水处理","硫化氢",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0049","废水处理","硫化氢",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0047","干燥","颗粒物",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0181","混粉机废气","颗粒物",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0179","磨粉机废气","颗粒物",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0040","缩合","挥发性有机物",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0040","缩合","颗粒物",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0228","无组织废气","氯化氢",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0227","无组织废气","氯化氢",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0226","无组织废气","氯化氢",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品原料药制造","MF0239","无组织废气","非甲烷总烃","密闭配套有效的管网送至净化系统,密闭并配备有效的废气捕集装置（如局部密闭罩、整体密闭罩、大容积密闭罩等）",null,"制药工业大气污染物排放标准GB37823—2019",null,"6mg/Nm3","/","/","/","/","/","/","监测点处一小时平均浓度值"]
["化学药品原料药制造","MF0239","无组织废气","非甲烷总烃","密闭配套有效的管网送至净化系统,密闭并配备有效的废气捕集装置（如局部密闭罩、整体密闭罩、大容积密闭罩等）",null,"制药工业大气污染物排放标准GB37823—2019",null,"20mg/Nm3","/","/","/","/","/","/","监测点处任意一次浓度值"]
["化学药品原料药制造","MF0180","振荡筛废气","颗粒物",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0142","包衣废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0140","包衣废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0139","包衣废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0141","包衣废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0123","分装废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0158","分装废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0157","分装废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0156","分装废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0159","分装废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0122","粉碎废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0154","粉针剂生产废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0155","粉针剂生产废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0153","粉针剂生产废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0152","粉针剂生产废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0151","粉针剂生产废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0121","干燥废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0119","干燥废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0116","干燥废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0115","干燥废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0113","干燥废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0114","干燥废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0110","干燥废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0117","干燥废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0118","干燥废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0120","干燥废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0111","干燥废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0112","干燥废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0125","混合废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0149","混合废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0150","混合废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0137","混合废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0136","混合废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0148","混合废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0147","混合废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0124","混合废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0233","配置废气","颗粒物",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/","加强车间通风"]
["化学药品制剂制造","MF0234","配置废气","颗粒物",null,null,"/",null,"/mg/Nm3","/","/","/","/","/","/","加强车间通风"]
["化学药品制剂制造","MF0134","筛分废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0132","筛分废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0133","筛分废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0135","筛分废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0189","水针剂生产废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0138","压片废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0131","制粒废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0130","制粒废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0129","制粒废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0127","制粒废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0126","制粒废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["化学药品制剂制造","MF0128","制粒废气","颗粒物","固体制剂车间废气处理设施",null,"/",null,"/mg/Nm3","/","/","/","/","/","/"]
["4、全厂无组织排放总计"]
["全厂无组织排放总计","污染物种类","年许可排放量限值（t/a）",{"$nulls":4},"申请特殊时段许可排放量限值"]
[null,null,"第一年","第二年","第三年","第四年","第五年"]
[null,"颗粒物","/ ","/ ","/ ","/ ","/ ","0 "]
[null,"SO2","/ ","/ ","/ ","/ ","/ ","0 "]
[null,"NOx","/ ","/ ","/ ","/ ","/ ","0 "]
[null,"VOCs","/ ","/ ","/ ","/ ","/ ","0 "]
["5、企业大气排放总许可量"]
["污染物种类","全厂有组织排放总计（t/a）",{"$nulls":4},"全厂无组织排放总计（t/a）",{"$nulls":4},"全厂合计（t/a）"]
[null,"第一年","第二年","第三年","第四年","第五年","第一年","第二年","第三年","第四年","第五年","第一年","第二年","第三年","第四年","第五年"]
["颗粒物","/","/","/","/","/","/","/","/","/","/","/ ","/ ","/ ","/ ","/ "]
["SO2","/","/","/","/","/","/","/","/","/","/","/ ","/ ","/ ","/ ","/ "]
["NOx","/","/","/","/","/","/","/","/","/","/","/ ","/ ","/ ","/ ","/ "]
["VOCs",5.904,5.904,5.904,5.904,5.904,"/","/","/","/","/","5.904 ","5.904 ","5.904 ","5.904 ","5.904 "]
["6、雨水排放口基本情况表"]
["排放口编号","排放口名称","排放口地理位置",null,"排水去向","排放规律","间歇式排放时段","受纳自然水体信息",null,"汇入受纳自然水体处地理坐标",null,"其他信息"]
[null,null,"经度","纬度",{"$nulls":3},"名称","受纳水体功能目标","经度","纬度"]
["DW002","雨水排放口","119度 10分 4.87秒","36度 47分 19.32秒","进入城市下水道（再入江河、湖、库）","间断排放，排放期间流量不稳定，但有规律，且不属于非周期性规律","下雨后15分钟","虞河","V类","119度 9分 4.25秒","36度 48分 24.26秒"]
["7、废水间接排放口基本情况表"]
["排放口编号","排放口名称","排放口地理坐标",null,"排放去向","排放规律","间歇排放时段","受纳污水处理厂信息"]
[null,null,"经度","纬度",{"$nulls":3},"名称","污染物种类",null,"排水协议规定的浓度限值(mg/L)",null,"国家或地方污染物排放标准浓度限值"]
["DW001","污水排放口","119度 10分 13.15秒","36度 47分 20.94秒","进入城市污水处理厂","间断排放，排放期间流量不稳定，但有周期性规律","9：00-11：00；15：00-21：00","山东高速环保科技有限公司","挥发酚",null,"/ mg/L",null,"/ mg/L"]
[{"$nulls":8},"pH值",null,"/",null,"6-9 "]
[{"$nulls":8},"五日生化需氧量",null,"/ mg/L",null,"10 mg/L"]
[{"$nulls":8},"硫化物",null,"/ mg/L",null,"/ mg/L"]
[{"$nulls":8},"色度",null,"/",null,"30 "]
[{"$nulls":8},"悬浮物",null,"/ mg/L",null,"10 mg/L"]
[{"$nulls":8},"总有机碳",null,"/ mg/L",null,"/ mg/L"]
[{"$nulls":8},"总锌",null,"/ mg/L",null,"1.0 mg/L"]
[{"$nulls":8},"化学需氧量",null,"/ mg/L",null,"50 mg/L"]
[{"$nulls":8},"总磷（以P计）",null,"/ mg/L",null,"1 mg/L"]
[{"$nulls":8},"总氮（以N计）",null,"/ mg/L",null,"15 mg/L"]
[{"$nulls":8},"二氯甲烷",null,"/ mg/L",null,"/ mg/L"]
[{"$nulls":8},"氨氮（NH3-N）",null,"/ mg/L",null,"5 mg/L"]
[{"$nulls":8},"急性毒性",null,"/ mg/L",null,"/ mg/L"]
["8、废水污染物排放执行标准表"]
["排放口编号","排放口名称","污染物种类",null,"国家或地方污染物排放标准",{"$nulls":3},"排水协议规定的浓度限值（如有）","环境影响评价审批意见要求","承诺更加严格排放限值","其他信息"]
[{"$nulls":4},"名称",null,null,"浓度限值"]
["DW001","污水排放口","硫化物",null,"污水排入城镇下水道水质标准GB/T 31962-2015",null,null,"1.0 mg/L","1.0 mg/L","1.0 mg/L","/ mg/L"]
["DW001","污水排放口","五日生化需氧量",null,"污水排入城镇下水道水质标准GB/T 31962-2015",null,null,"350 mg/L","350 mg/L","350 mg/L","/ mg/L"]
["DW001","污水排放口","化学需氧量",null,"污水排入城镇下水道水质标准GB/T 31962-2015",null,null,"500 mg/L","500 mg/L","500 mg/L","/ mg/L"]
["DW001","污水排放口","氨氮（NH3-N）",null,"污水排入城镇下水道水质标准GB/T 31962-2015",null,null,"45 mg/L","45 mg/L","45 mg/L","/ mg/L"]
["DW001","污水排放口","悬浮物",null,"污水排入城镇下水道水质标准GB/T 31962-2015",null,null,"400 mg/L","400 mg/L","400 mg/L","/ mg/L"]
["DW001","污水排放口","色度",null,"污水排入城镇下水道水质标准GB/T 31962-2015",null,null,"64 ",64,64,"/","单位为倍"]
["DW001","污水排放口","挥发酚",null,"污水排入城镇下水道水质标准GB/T 31962-2015",null,null,"1 mg/L","1 mg/L","1 mg/L","/ mg/L"]
["DW001","污水排放口","总锌",null,"污水排入城镇下水道水质标准GB/T 31962-2015",null,null,"5 mg/L","5 mg/L","5 mg/L","/ mg/L"]
["DW001","污水排放口","pH值",null,"污水排入城镇下水道水质标准GB/T 31962-2015",null,null,"6.5-9.5 ","6.5-9.5","6.9-9.5","/"]
["DW001","污水排放口","总氮（以N计）",null,"污水排入城镇下水道水质标准GB/T 31962-2015",null,null,"70 mg/L","70 mg/L","70 mg/L","/ mg/L"]
["DW001","污水排放口","二氯甲烷",null,"/",null,null,"/ mg/L","/ mg/L","/ mg/L","/ mg/L"]
["DW001","污水排放口","总有机碳",null,"/",null,null,"/ mg/L","/ mg/L","/ mg/L","/ mg/L"]
["DW001","污水排放口","急性毒性",null,"/",null,null,"/ mg/L","/ mg/L","/ mg/L","/ mg/L"]
["DW001","污水排放口","总磷（以P计）",null,"污水排入城镇下水道水质标准GB/T 31962-2015",null,null,"8 mg/L","8 mg/L","8 mg/L","/ mg/L"]
["9、申请排放信息"]
["（1）主要排放口"]
["排放口编号","排放口名称","污染物种类","申请排放浓度限值","申请年排放量限值（t/a）",{"$nulls":4},"申请特殊时段排放量限值"]
[{"$nulls":4},"第一年","第二年","第三年","第四年","第五年"]
["DW001","污水排放口","硫化物","/mg/L","/","/","/","/","/","/"]
["DW001","污水排放口","化学需氧量","500mg/L",50.224,50.224,50.224,50.224,50.224,"/"]
["DW001","污水排放口","总氮（以N计）","70mg/L",7.031,7.031,7.031,7.031,7.031,"/"]
["DW001","污水排放口","挥发酚","1mg/L","/","/","/","/","/","/"]
["DW001","污水排放口","总锌","5mg/L","/","/","/","/","/","/"]
["DW001","污水排放口","悬浮物","400mg/L","/","/","/","/","/","/"]
["DW001","污水排放口","pH值","6.5-9.5","/","/","/","/","/","/"]
["DW001","污水排放口","总磷（以P计）","8mg/L","/","/","/","/","/","/"]
["DW001","污水排放口","急性毒性","/mg/L","/","/","/","/","/","/"]
["DW001","污水排放口","氨氮（NH3-N）","45mg/L",4.52,4.52,4.52,4.52,4.52,"/"]
["DW001","污水排放口","五日生化需氧量","350mg/L","/","/","/","/","/","/"]
["DW001","污水排放口","色度",64,"/","/","/","/","/","/"]
["DW001","污水排放口","二氯甲烷","/mg/L","/","/","/","/","/","/"]
["DW001","污水排放口","总有机碳","/mg/L","/","/","/","/","/","/"]
["主要排放口合计",null,null,"CODcr",50.224,50.224,50.224,50.224,50.224,"/ "]
[{"$nulls":3},"氨氮",4.52,4.52,4.52,4.52,4.52,"/ "]
[{"$nulls":3},"总氮（以N计）",7.031,7.031,7.031,7.031,7.031,"/ "]
["（2）一般排放口"]
["排放口编号","排放口名称","污染物种类","申请排放浓度限值","申请年排放量限值（t/a）",{"$nulls":4},"申请特殊时段排放量限值"]
[{"$nulls":4},"第一年","第二年","第三年","第四年","第五年"]
["一般排放口合计",null,null,"CODcr",{"$nulls":5},"/ "]
[{"$nulls":3},"氨氮",{"$nulls":5},"/ "]
[{"$nulls":3},"总氮（以N计）",{"$nulls":5},"/ "]
["（3）全厂排放口总计"]
["全厂排放口总计","污染物种类","申请年排放量限值（t/a）",{"$nulls":4},"申请特殊时段排放量限值"]
[null,null,"第一年","第二年","第三年","第四年","第五年"]
[null,"CODcr",50.224,50.224,50.224,"50.224 ","50.224 ","/ "]
[null,"氨氮",4.52,4.52,4.52,"4.52 ",4.52,"/ "]
[null,"总氮（以N计）",7.031,7.031,"7.031 ",7.031,"7.031 ","/ "]
[]
[]
["10、固体废物排放信息及委托利用、委托处置"]
["行业类别","固体废物来源","固体废物名称","固体废物种类","固体废物类别","固体废物描述",null,null,"固体废物产生量（t/a）","处理方式","处理去向",{"$nulls":4},"其他信息"]
[{"$nulls":10},"自行贮存量（t/a）","自行利用处置（t/a）","转移量（t/a）",null,"排放量（t/a）"]
[{"$nulls":12},"委托利用量","委托处置量"]
["化学药品原料药制造","公用单元","废活性炭","其它固体废物（含半液态、液态废物）","一般工业固体废物","公用单元纯水制备设施产生",null,null,3,"委托利用",0,0,3,0,0]
[null,"卡托普利生产线","废脱色过滤介质及残渣","危险废物","危险废物","卡托普利生产过程产生的废脱色过滤介质及残渣，属于危险废物，代码为271-003-02。",null,null,6,"委托处置",0,0,0,6,0]
[null,"卡托普利生产线","废包装（乳糖、淀粉、活性炭等包装袋、瓶）","废包装（乳糖、淀粉、活性炭等包装袋、瓶）","一般工业固体废物","废生产过程中使用的原辅材料包装（乳糖、淀粉、活性炭等包装袋、瓶）废弃，为一般固体废弃物。",null,null,3,"委托利用",0,0,3,0,0]
[null,"卡托普利生产线","废包装","危险废物","危险废物","原辅材料使用后废弃的具有环境危害性的包装物，为危险废物，代码为900-041-49。",null,null,0.5,"委托处置",0,0,0,0.5,0]
[null,"乙酰谷酰氨生产线","有机废液","危险废物","危险废物","乙酰谷酰氨生产线生产的16中原料药生产过程产生的有机废液，属于危险废物，代码为900-403-06",null,null,67.14,"委托处置",0,0,0,67.14,0]
[null,"乙酰谷酰氨生产线","废脱色过滤介质及残渣","危险废物","危险废物","乙酰谷酰氨生产线生产的16种原料药生产过程中产生的废脱色过滤介质及残渣，属于危险废物，代码为：271-003-02。",null,null,21.78,"委托处置",0,0,0,21.78,0]
[null,"公用单元","实验室废液","危险废物","危险废物","实验室检验过程产生的废液，为危险废物，代码为900-047-49。",null,null,0.02,"委托处置",0,0,0,0.02,0]
[null,"公用单元","污水处理站污泥","危险废物","危险废物","污水处理过程产生的污泥，为危险废物，代码为：900-410-06。",null,null,160,"委托处置",0,0,0,160,0]
["化学药品原料药制造","公用单元","废活性炭","危险废物","危险废物","污水处理站废气处理设施产生的废活性炭，为危险废物，代码为：900-041-49。",null,null,0.5,"委托处置",0,0,0,0.5,0]
[]
["固体废物来源","固体废物名称","固体废物类别","委托单位名称",null,"危险废物利用和处置单位危险废物经营许可证编号"]
["公用单元","废活性炭","一般工业固体废物","山东信洁物业管理公司"]
["公用单元","废活性炭","危险废物","山东环沃环保科技有限公司",null,"滨州危废临07号"]
["公用单元","实验室废液","危险废物","山东环沃环保科技有限公司",null,"滨州危废临07号"]
["公用单元","污水处理站污泥","危险废物","山东环沃环保科技有限公司",null,"滨州危废临07号"]
["卡托普利生产线","废包装","危险废物","山东环沃环保科技有限公司",null,"滨州危废临07号"]
["卡托普利生产线","废包装（乳糖、淀粉、活性炭等包装袋、瓶）","一般工业固体废物","山东信洁物业管理公司"]
["卡托普利生产线","废脱色过滤介质及残渣","危险废物","山东环沃环保科技有限公司",null,"滨州危废临07号"]
["乙酰谷酰氨生产线","废脱色过滤介质及残渣","危险废物","山东环沃环保科技有限公司",null,"滨州危废临07号"]
["乙酰谷酰氨生产线","有机废液","危险废物","山东环沃环保科技有限公司",null,"滨州危废临07号"]
[]
["三、产排污节点、污染物及污染治理设施"]
["（1）废气产排污节点、污染物及污染治理设施信息表"]
["产污设施编号","产污设施名称","对应产污环节名称","污染物种类","排放形式","污染治理设施",{"$nulls":3},"有组织排放口编号","有组织排放口名称","排放口设置是否符合要求","排放口类型","其他信息"]
[{"$nulls":5},"污染防治设施编号","污染防治设施名称","污染治理设施工艺","是否为可行技术"]
["MF0047","双锥回转真空干燥机","干燥废气","颗粒物","有组织","TA003","工艺含尘废气治理设施","袋式除尘","是","DA001","废气排放口","是","主要排放口"]
[null,null,"干燥废气","挥发性有机物,总挥发性有机物","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0044","搪玻璃反应罐","反应废气","挥发性有机物,总挥发性有机物,氯化氢","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0045","搪玻璃反应罐","反应废气","挥发性有机物,总挥发性有机物,氯化氢","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0040","搪玻璃反应罐","反应废气","挥发性有机物,氯化氢,总挥发性有机物","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0041","不锈钢反应罐","反应废气","挥发性有机物,总挥发性有机物,氯化氢","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0192","水解酸化池","污水处理设施","挥发性有机物,氨（氨气）,硫化氢,臭气浓度,苯系物","有组织","TA005","废水处理站废气治理设施","光催化氧化,生物洗涤,活性炭吸附","是","DA003","污水处理设施废气排放口","是","主要排放口"]
["MF0193","二沉池","污水处理设施","挥发性有机物,臭气浓度,氨（氨气）,硫化氢,苯系物","有组织","TA005","废水处理站废气治理设施","光催化氧化,生物洗涤,活性炭吸附","是","DA003","污水处理设施废气排放口","是","主要排放口"]
["MF0056","搪玻璃反应罐","反应废气","挥发性有机物,总挥发性有机物,氯化氢","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0054","搪玻璃反应罐","反应废气","挥发性有机物,总挥发性有机物,氯化氢","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0055","搪玻璃反应罐","反应废气","挥发性有机物,总挥发性有机物,氯化氢","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0038","三足式人工上卸料离心机","离心废气","颗粒物,挥发性有机物,总挥发性有机物","有组织","TA001","工艺有机废气治理设施","水洗,碱吸收","是","DA001","废气排放口","是","主要排放口"]
["MF0057","搪玻璃反应罐","反应废气","挥发性有机物,总挥发性有机物,氯化氢","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0039","双锥干燥器","双锥干燥器废气","颗粒物,挥发性有机物,总挥发性有机物","有组织","TA001","工艺有机废气治理设施","水洗,碱吸收","是","DA001","废气排放口","是","主要排放口"]
["MF0053","搪玻璃反应罐","反应废气","挥发性有机物,总挥发性有机物,氯化氢","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0049","混凝沉淀池","污水处理设施","挥发性有机物,臭气浓度,氨（氨气）,硫化氢,苯系物","有组织","TA005","废水处理站废气治理设施","光催化氧化,生物洗涤,活性炭吸附","是","DA003","污水处理设施废气排放口","是","主要排放口"]
["MF0058","搪玻璃反应罐","反应废气","挥发性有机物,总挥发性有机物,氯化氢","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0050","曝气生物滤池","污水处理废气","挥发性有机物,臭气浓度,氨（氨气）,硫化氢,苯系物","有组织","TA005","废水处理站废气治理设施","光催化氧化,生物洗涤,活性炭吸附","是","DA003","污水处理设施废气排放口","是","主要排放口"]
["MF0108","振荡筛","振荡筛废气","颗粒物","有组织","TA003","工艺含尘废气治理设施","袋式除尘","是","DA001","废气排放口","是","主要排放口"]
["MF0051","中和池","污水处理设施","挥发性有机物,臭气浓度,氨（氨气）,硫化氢,苯系物","有组织","TA005","废水处理站废气治理设施","光催化氧化,生物洗涤,活性炭吸附","是","DA003","污水处理设施废气排放口","是","主要排放口"]
["MF0048","混粉机","混粉机废气","颗粒物","有组织","TA003","工艺含尘废气治理设施","袋式除尘","是","DA001","废气排放口","是","主要排放口"]
["MF0140","包衣机","包衣废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0109","磨粉机","磨粉机废气","颗粒物","有组织","TA003","工艺含尘废气治理设施","袋式除尘","是","DA001","废气排放口","是","主要排放口"]
["MF0141","包衣机","包衣废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0097","钛棒过滤器","过滤废气","挥发性有机物,总挥发性有机物,氯化氢","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0094","钛棒过滤器","过滤废气","氯化氢,挥发性有机物,总挥发性有机物","有组织","TA004","工艺有机废气治理设施","水洗,冷凝","是","DA001","废气排放口","是","主要排放口"]
["MF0139","包衣机","包衣废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0035","搪玻璃反应罐","反应废气","挥发性有机物,总挥发性有机物","有组织","TA001","工艺有机废气治理设施","水洗,碱吸收","是","DA001","废气排放口","是","主要排放口"]
["MF0098","钛棒过滤器","过滤废气","挥发性有机物,总挥发性有机物,氯化氢","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0142","包衣机","包衣废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0088","离心机","离心机废气","挥发性有机物,总挥发性有机物","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0042","搪玻璃反应罐","反应废气","挥发性有机物,总挥发性有机物,氯化氢","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0099","离心机","离心机废气","挥发性有机物,总挥发性有机物","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0110","沸腾床","干燥废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0103","离心机","离心机废气","挥发性有机物,总挥发性有机物","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0100","离心机","离心机废气","挥发性有机物,总挥发性有机物","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0096","钛棒过滤器","过滤废气","挥发性有机物,总挥发性有机物,氯化氢","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0095","钛棒过滤器","过滤废气","挥发性有机物,总挥发性有机物,氯化氢","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0111","热风循环烘箱","干燥废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0046","离心机","离心机废气","挥发性有机物,总挥发性有机物","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0101","离心机","离心机废气","挥发性有机物,总挥发性有机物","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0104","离心机","离心机废气","挥发性有机物,总挥发性有机物","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0102","离心机","离心机废气","挥发性有机物,总挥发性有机物","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0136","高效湿法混合制粒机","混合废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0060","回收卡托普利干燥器","干燥废气","颗粒物","有组织","TA003","工艺含尘废气治理设施","袋式除尘","是","DA001","废气排放口","是","主要排放口"]
[null,null,"干燥废气","挥发性有机物,总挥发性有机物","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0127","振荡筛","制粒废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0059","双锥回转真空干燥机","干燥废气","颗粒物","有组织","TA003","工艺含尘废气治理设施","袋式除尘","是","DA001","废气排放口","是","主要排放口"]
[null,null,"干燥废气","挥发性有机物,总挥发性有机物","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0132","整粒机","筛分废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0085","浓盐酸计量罐","计量废气","氯化氢","有组织","TA004","工艺酸碱废气治理设施","水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0128","振荡筛","制粒废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0084","浓盐酸计量罐","计量废气","氯化氢","有组织","TA004","工艺酸碱废气治理设施","水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0133","整粒机","筛分废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0129","振荡筛","制粒废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0075","盐酸计量罐","计量废气","氯化氢","有组织","TA004","工艺酸碱废气治理设施","水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0135","整粒机","筛分废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0134","整粒机","筛分废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0131","振荡筛","制粒废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0076","盐酸计量罐","计量废气","氯化氢","有组织","TA004","工艺酸碱废气治理设施","水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0130","振荡筛","制粒废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0077","盐酸计量罐","计量废气","氯化氢","有组织","TA004","工艺酸碱废气治理设施","水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0137","高速混合制粒机","混合废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0126","振荡筛","制粒废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0078","盐酸计量罐","计量废气","氯化氢","有组织","TA004","工艺酸碱废气治理设施","水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0138","全自动高速压片机","压片废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0125","三维运动混合机","混合废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0124","三维运动混合机","混合废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0123","全自动硬胶囊填充机","分装废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0147","一维运动混合机","混合废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0148","一维运动混合机","混合废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0150","一维运动混合机","混合废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0149","一维运动混合机","混合废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0122","不锈钢粉碎机","粉碎废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0074","盐酸计量罐","计量废气","氯化氢","有组织","TA001","工艺酸碱废气治理设施","水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0156","分装机","分装废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0157","分装机","分装废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0158","分装机","分装废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0159","分装机","分装废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0087","浓盐酸计量罐","计量废气","氯化氢","有组织","TA001","工艺酸碱废气治理设施","水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0155","电热恒温鼓风干燥箱","粉针剂生产废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0086","浓盐酸计量罐","计量废气","氯化氢","有组织","TA001","工艺酸碱废气治理设施","水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0151","二合一装置","粉针剂生产废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0154","旋转除湿器","粉针剂生产废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0153","不锈钢恒温烘箱","粉针剂生产废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0152","二合一装置","粉针剂生产废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0105","结晶罐","结晶罐废气","挥发性有机物,总挥发性有机物,氯化氢","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0189","干燥灭菌器","水针剂生产废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0107","结晶罐","结晶罐废气","挥发性有机物,总挥发性有机物,氯化氢","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0082","母液回收罐","母液回收废气","挥发性有机物,总挥发性有机物","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0106","结晶罐","结晶罐废气","挥发性有机物,总挥发性有机物","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0083","母液回收罐","母液回收废气","挥发性有机物,总挥发性有机物","有组织","TA004","工艺有机废气治理设施","冷凝,水洗","是","DA001","废气排放口","是","主要排放口"]
["MF0162","反应接受罐","反应废气","挥发性有机物,总挥发性有机物","有组织","TA001","工艺有机废气治理设施","水洗,碱吸收","是","DA001","废气排放口","是","主要排放口"]
["MF0164","脱色槽","脱色废气","挥发性有机物,总挥发性有机物","有组织","TA001","工艺有机废气治理设施","水洗,碱吸收","是","DA001","废气排放口","是","主要排放口"]
["MF0165","中转槽","反应废气","挥发性有机物,总挥发性有机物","有组织","TA001","工艺有机废气治理设施","水洗,碱吸收","是","DA001","废气排放口","是","主要排放口"]
["MF0161","离心母液槽","反应废气","挥发性有机物,总挥发性有机物","有组织","TA001","工艺有机废气治理设施","水洗,碱吸收","是","DA001","废气排放口","是","主要排放口"]
["MF0160","离心母液槽","反应废气","挥发性有机物,总挥发性有机物","有组织","TA001","工艺有机废气治理设施","水洗,碱吸收","是","DA001","废气排放口","是","主要排放口"]
["MF0037","反应接受罐","反应废气","挥发性有机物,总挥发性有机物","有组织","TA001","工艺有机废气治理设施","水洗,碱吸收","是","DA001","废气排放口","是","主要排放口"]
["MF0174","甲醇溶解罐","溶解废气","甲醇,挥发性有机物,总挥发性有机物","有组织","TA001","工艺有机废气治理设施","水洗,碱吸收","是","DA001","废气排放口","是","主要排放口"]
["MF0175","异丙醇计量罐","计量废气","异丙醇,挥发性有机物,总挥发性有机物","有组织","TA001","工艺有机废气治理设施","水洗,碱吸收","是","DA001","废气排放口","是","主要排放口"]
["MF0178","结晶罐","结晶罐废气","挥发性有机物,总挥发性有机物","有组织","TA001","工艺有机废气治理设施","水洗,碱吸收","是","DA001","废气排放口","是","主要排放口"]
["MF0176","结晶罐","结晶罐废气","挥发性有机物,总挥发性有机物","有组织","TA001","工艺有机废气治理设施","水洗,碱吸收","是","DA001","废气排放口","是","主要排放口"]
["MF0177","结晶罐","结晶罐废气","挥发性有机物,总挥发性有机物","有组织","TA001","工艺有机废气治理设施","水洗,碱吸收","是","DA001","废气排放口","是","主要排放口"]
["MF0166","三足式人工上卸料离心机","离心废气","挥发性有机物,总挥发性有机物","有组织","TA001","工艺有机废气治理设施","水洗,碱吸收","是","DA001","废气排放口","是","主要排放口"]
["MF0169","钛棒过滤器","过滤废气","挥发性有机物,总挥发性有机物","有组织","TA001","工艺有机废气治理设施","水洗,碱吸收","是","DA001","废气排放口","是","主要排放口"]
["MF0170","钛棒过滤器","过滤废气","挥发性有机物,总挥发性有机物","有组织","TA001","工艺有机废气治理设施","水洗,碱吸收","是","DA001","废气排放口","是","主要排放口"]
["MF0167","过滤打料泵","过滤废气","挥发性有机物,总挥发性有机物","有组织","TA001","工艺有机废气治理设施","水洗,碱吸收","是","DA001","废气排放口","是","主要排放口"]
["MF0182","蒸馏罐","溶剂回收废气","挥发性有机物,甲醇,乙醇,丙酮,四氢呋喃,正己烷,甲酸乙酯,乙酸乙酯,氯乙酸乙酯,三氯甲烷,二氯甲烷,总挥发性有机物","有组织","TA001","工艺有机废气治理设施","水洗,碱吸收","是","DA001","废气排放口","是","主要排放口"]
[null,null,"蒸馏废气","二氯甲烷,甲醇,乙醇,四氢呋喃,乙酸乙酯,丙酮,氯化氢,正己烷,挥发性有机物,总挥发性有机物","有组织","TA001","工艺有机废气治理设施","水洗,碱吸收","是","DA001","废气排放口","是","主要排放口"]
["MF0194","危险废物暂存间","危废暂存废气","挥发性有机物,臭气浓度,硫化氢,氨（氨气）","有组织","TA005","废水处理站废气治理设施","光催化氧化,生物洗涤,活性炭吸附","是","DA003","污水处理设施废气排放口","是","主要排放口"]
["MF0180","振荡筛","振荡筛废气","颗粒物","无组织","/"]
["MF0181","混粉机","混粉机废气","颗粒物","无组织","/"]
["MF0179","磨粉机","磨粉机废气","颗粒物","无组织","/"]
["MF0228","常压罐","无组织废气","氯化氢","无组织","/"]
["MF0226","常压罐","无组织废气","氯化氢","无组织","/"]
["MF0227","常压罐","无组织废气","氯化氢","无组织","/"]
["MF0116","热风循环烘箱","干燥废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0113","热风循环烘箱","干燥废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0114","热风循环烘箱","干燥废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0117","热风循环烘箱","干燥废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0233","配制罐","配置废气","颗粒物","无组织","/",{"$nulls":7},"加强车间通风"]
["MF0234","配制罐","配置废气","颗粒物","无组织","/",{"$nulls":7},"加强车间通风"]
["MF0119","热风循环烘箱","干燥废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0118","热风循环烘箱","干燥废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0115","热风循环烘箱","干燥废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0120","热风循环烘箱","干燥废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0121","热风循环烘箱","干燥废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["MF0112","热风循环烘箱","干燥废气","颗粒物","无组织","TA006","固体制剂车间废气处理设施","高效过滤器","是"]
["（2）废水类别、污染物及污染治理设施信息表"]
["行业类别","废水类别","污染物种类","污染治理设施",{"$nulls":3},"排放去向","排放方式","排放规律","排放口编号","排放口名称","排放口设置是否符合要求","排放口类型"]
[{"$nulls":3},"污染治理设施编号","污染治理设施名称","污染治理设施工艺","是否为可行技术"]
["化学药品原料药制造","废气处理设施废水,主生产过程排水-合成废水,主生产过程排水-设备冲洗水,循环冷却水排水,中水回用系统排水,水环真空泵排水,制水排水,蒸馏设备冷凝水,初期雨水,生活污水","化学需氧量,氨氮（NH3-N）,总氮（以N计）,总磷（以P计）,硫化物,急性毒性,色度,悬浮物,pH值,挥发酚,五日生化需氧量,总锌,二氯甲烷,总有机碳","TW001","综合废水处理设施","混凝沉淀,水解酸化,曝气生物滤池（BAF）,调节,二沉池","是","进入城市污水处理厂","间接排放","间断排放，排放期间流量不稳定，但有周期性规律","DW001","污水排放口","是","主要排放口-总排口"]
["化学药品制剂制造","生产单元废水,公用单元废水,生活污水,初期雨水","化学需氧量,氨氮（NH3-N）,总氮（以N计）,总磷（以P计）,总有机碳,五日生化需氧量,悬浮物,急性毒性,pH值","TW001","综合废水处理站","混凝沉淀,水解酸化,曝气生物滤池，调节池，二沉池","是","进入城市污水处理厂","间接排放","间断排放，排放期间流量不稳定，但有周期性规律","DW001","污水排放口","是","主要排放口-总排口"]
["四、建设项目环境影响评价及其他环境保护行政许可情况"]
["潍环审字（2011）10号"]
["寒环审表字【2018】94号"]
["寒环审表字[2019]101号"]
["寒环审表字[2019]61号"]
["潍环寒评函【2020】1号"]
["五、突发环境事件应急预案"]
["备案编号：370703-2021-096-L"]